**J/105 Inspection Check List**

Boat Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Hull #: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Measurer: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_ Fuel = ½ tank or more as per gauge

\_\_\_\_\_ Weight Certificate – verify that weight certificate matches the boat

\_\_\_\_\_Verify that tags on sails match those declared for the event

\_\_\_\_\_ Mast Step (no evidence of modification of the mast or step)

\_\_\_\_\_ Taut Lifelines (see CR 7.11)

\_\_\_\_\_ Anchor w/attached chain and/or rode

\_\_\_\_\_ all USCG-required safety items (including flares, foghorn, and fire extinguishers)

\_\_\_\_\_ 1st aid kit, 1 bucket, 2 flashlights

\_\_\_\_\_ 2 main cabin berth cushions

\_\_\_\_\_ Standard companionway board(s)

\_\_\_\_\_ Life sling, "man-overboard module" or horseshoe life ring; cannot interfere with swim ladder.

\_\_\_\_\_ Basic navigation gear (e.g., chart book, ruler, dividers, tide book & rulebook)

\_\_\_\_\_ Tool kit

\_\_\_\_\_ Handheld or installed VHF and GPS

\_\_\_\_\_ Radar reflector

\_\_\_\_\_ Emergency tiller that fits. Advise if it doesn’t.

\_\_\_\_\_ Standard cooler, in standard location

\_\_\_\_\_ 1 standard-sized battery in standard location (see CR 5.3.20)

\_\_\_\_\_ Boat hook

\_\_\_\_\_ 2 dock lines and 2 fenders

\_\_\_\_\_ Bosun’s chair or climbing harness

\_\_\_\_\_ Standard equipment as required by the CR and Weight Certificate